**Lab 4:**Q1.2:  
We can also use write syscall, that also returns EFAULT if the addr is not mapped in the memory

Q1.4:

We would make prefetch a non-observable hint for user mode so it must not cause page-table walks that leave observable microarchitectural traces that will reveal the mapped addresses to the user, for example, we can check permissions of the user to scan the pages.